**ABSTRACT**

## ABSTRACT

Atmospheric gravity waves play a critical role in the vertical coupling of energy and momentum across different layers of the atmosphere. This study focuses on the detection and spectral analysis of convection-triggered gravity waves using ground-based LIDAR remote sensing data obtained from the National Atmospheric Research Laboratory (NARL), Gadanki. Over an 8-week research internship under the Summer Research Fellowship Programme (SRFP), LiDAR backscatter profiles were analyzed to extract temporal and spatial variations in atmospheric structures.

More than 800 files containing LiDAR returns were pre-processed and combined to form a multi-dimensional dataset. Range-Time Intensity (RTI) plots were generated to visualize wave signatures, and altitude-specific time series were extracted to perform Fast Fourier Transform (FFT)-based spectral analysis. The dominant frequencies identified across multiple altitude bins revealed consistent low-frequency oscillations, confirming the presence of gravity waves typically associated with convective activity.

The analysis demonstrated that LiDAR remote sensing is an effective tool for capturing the vertical propagation characteristics of gravity waves in the lower and middle atmosphere. The extracted wave periods matched theoretical expectations, and the results contribute valuable insights into mesoscale atmospheric dynamics. This work lays the groundwork for future research using advanced filtering techniques and multi-instrumental observations to enhance the detection accuracy and understand wave source mechanisms in the tropical atmosphere.

.

**LIST OF TABLES**

|  |  |  |
| --- | --- | --- |
| **S. No** | **Name** | **Page. No** |
| 1 | Summary of FFT Results Across Altitudes | 12 |
| 2 | Hardware Specification | 14 |
| 3 | Software Specification | 14 |
| 4 | Phase Difference at Various Altitudes | 29 |
| 5 | Frequency Findings | 30 |
| 6 | Interpretation of FFT Results | 30 |

**LIST OF FIGURES**

|  |  |  |
| --- | --- | --- |
| **S. No** | **Name** | **Page. No** |
| 1 | Flow Chart | 9 |
| 2 | Sample Licel Binary File Header Information | 9 |
| 3 | Header Information | 12 |
| 4 | RTI Plot Showing Gravity Wave Signatures | 17 |
| 5 | FFT-Based Spectral Analysis at Multiple Altitudes | 19 - 22 |
| 6 | Signal Intensity vs Time at 385 m (Bin 100) | 23 |
| 7 | Signal Intensity vs Time at 387.7 m (Bin 127) | 24 |
| 8 | Signal Intensity vs Time at 390.4 m (Bin 154) | 24 |
| 9 | Signal Intensity vs Time at 393.1 m (Bin 181) | 24 |
| 10 | Signal Intensity vs Time at 395.8 m (Bin 208) | 25 |
| 11 | Signal Intensity vs Time at 398.5 m (Bin 235) | 25 |
| 12 | Signal Intensity vs Time at 401.2 m (Bin 262) | 25 |
| 13 | Signal Intensity vs Time at 403.9 m (Bin 289) | 26 |
| 14 | Signal Intensity vs Time at 406.6 m (Bin 316) | 26 |
| 15 | Signal Intensity vs Time at 409.3 m (Bin 343) | 26 |
| 16 | Variation of Phase Difference with Altitude | 29 |